**200 W Frameless BLDC Motor**



|  |
| --- |
| Basic Motor Parameters |
| Rated Power | W | 200 |
| Rated Speed | rpm | 6000 |
| Rated Torque | Nm | 0.25 |
| Rated Current | A | 2.2 |
| Rated Voltage | V | 120 |
| No-Load Speed | rpm | 8500 |
| Max. Efficiency | % | ~83 |
| Electrical Parameters |
| Number of Phases |  | 3 |
| Number of Poles |  | 8 |
| Torque Constant (KT) | Nm/A | 0.124 |
| Back EMF Constant (KE) | Vs/rad | 0.13 |
| Terminal Resistance Phase to Phase (±%10) | mΩ | 1.9 |
| Terminal Inductance Phase to Phase (±%30) | mH | 1.4 |
| Thermal Data |
| Ambient Temperature | °C | -40...+85 |
| Max. Winding Temperature | °C | +155 |
| Physical Parameters |
| Outer Diameter | mm | 37.780 |
| Shaft Diameter | mm | N/A |
| Max. Lenght | mm | 75.57 |
| Weight | gr | 100 |
| Motor Connection |
| N/A | N/A |
| Sensor Connection |
| N/A | N/A |
| Connector Articles |
| Power | N/A |
| Signal | N/A |