**DM-G35 Drone Motor**



|  |
| --- |
| Basic Motor Parameters |
| Throttle | % | 60 |
| Max. Thrust | kg | 5.1 |
| Recommended Takeoff Weight | kg | 2-2,5 |
| Torque | Nm | 0.37 |
| KV Rating | rpm/V | 900 |
| Bus Voltage | S | 6S |
| Max. Efficiency | % | 90 |
| Operating Current | A | 23 |
| Rated Speed | rpm | 9500 |
| Propeller Force Efficiency | g/W | 4.3 |
| Electrical Parameters |
| Number of Phases |  | 3 |
| Number of Poles |  | 14 |
| Terminal Resistance Phase to Phase (±%10) | mΩ | 45 |
| Terminal Inductance Phase to Phase (±%30) | mH | 30 |
| Thermal Data |
| Ambient Temperature | °C | -40...+85 |
| Max. Winding Temperature | °C | +155 |
| Physical Parameters |
| Outer Diameter | mm | 37.1 |
| Shaft Diameter | mm | M5 |
| Max. Lenght | mm | 47.8 |
| Weight | gr | 121 |
| Motor Connection |
| U | Black |
| V | Black |
| W | Black |
| Sensor Connection |
| N/A | N/A |
| Connector Articles |
| Power | N/A |
| Signal | N/A |
| Propeller Info (Recommended) |
| Diameter | 10” |
| Pitch | 5” |